**Kindly note that in Q related to Thevenin's ckt,**

**value of Rth = 3 ohms.**

**Accordingly Current flowing through the required register R=7ohm is I7=1Amp.**